#ifndef API_GLOBAL__H
#define API_GLOBAL__H

#include <avr/pgmspace.h>
#include "OWIDeviceSpecific.h"
#include "OWIHighLevelFunctions.h"
#include "OWIBitFunctions.h"
#include "api_define.h"

/* Canapi.h*/

//char tmp_str[BUFFER_SIZE];

extern char canString[MAX_LENGTH_CAN_DATA];
extern char decrypt_uartString[BUFFER_SIZE];
extern char ring_buffer[MAX_INPUT][MAX_LENGTH_CAN_DATA];/*variable for storage all received CAN data*/
extern char setParameter[MAX_PARAMETER][MAX_LENGTH_PARAMETER]; /*storage of cut string */
extern char *ptr_setParameter[MAX_PARAMETER];
extern char uart_message_string[BUFFER_SIZE];
extern char message[BUFFER_SIZE];
extern char uartString[BUFFER_SIZE]; /* variable for storage received a complete string via UART */
extern char keepAliveString[15];

extern int8_t can_init; /* variable to call CAN_Init function*/
extern int8_t timer0_init; /* variable to call Timer0_Init function*/
extern int8_t timer0A_init;/* variable to call Timer0A_Init function*/

extern uint8_t can_errorCode; /* error code for CAN-communication */
extern uint8_t general_errorCode; /*general error code */
extern uint8_t mailbox_errorCode; /* error code for Message Object Block */
extern uint8_t uart_errorCode; /* error code for UART-communication */

extern volatile unsigned char BufferFull;/*variable for UART Interrupt*/
extern volatile unsigned char canReady; /* variable for CAN ISR */

extern volatile unsigned char timer0Ready;/*variable for Timer  Interrupt*/
extern volatile unsigned char timer1Ready;/*variable for Timer  Interrupt*/
extern volatile unsigned char timer0AReady;/*variable for Timer0 Output Compare A  Interrupt*/
extern volatile unsigned char timer0ASchedulerReady;/*variable for Timer0 Output Compare A  Interrupt*/
extern volatile unsigned char uartReady;/*variable for UART Interrupt*/

extern uint8_t mob; /*variable  for Message Object Block in the interrupt routine*/
extern unsigned char nextCharPos;/* variable for the storage of data in serial string variable */

extern uint16_t subscribe_ID[MAX_LENGTH_SUBSCRIBE];
extern uint16_t subscribe_mask[MAX_LENGTH_SUBSCRIBE];

extern uint8_t ptr_buffer_in; /*pointer for write in ring_buffer*/
extern uint8_t ptr_buffer_out; /*pointer for read in ring_buffer*/
extern uint8_t ptr_subscribe; /* pointer of variable subscribe_ID and subscribe_mask */

extern uint8_t flag_pingActive; /* flag for PING mechanism */

extern const uint8_t serial_error_number[] ;
extern const char *serial_error[] PROGMEM;

extern const uint8_t can_error_number[];
extern const char *can_error[] PROGMEM;

extern const uint8_t mob_error_number[] ;
extern const char *mob_error[] PROGMEM;

extern const uint16_t general_error_number[];
extern const char *general_error[] PROGMEM;

extern char currentCommandKeyword[MAX_LENGTH_KEYWORD];/*variable to store current command keyword e.g. "SEND"*/
extern char currentResponseKeyword[MAX_LENGTH_KEYWORD];/*variable to store current command keyword e.g. "RECV"*/

extern uint16_t Voltages[8];/* current supply voltages of the board*/

/*variable to store values*/
extern char tmp_str[BUFFER_SIZE];

extern uint8_t cur_state;
extern uint8_t usercommand;

extern volatile uint16_t thigh;/*the maximum gas pressure*/
extern volatile uint16_t tlow;/*the minimum gas pressure*/

extern uint8_t res0, res1, res2, res3; /*parameter back to reading the voltage on ADC-channel*/

extern uint8_t NumDevicesFound;

extern uint8_t owi_IDs[NUM_DEVICES][8]; /*Global variable to store the ID numbers of ALL devices*/
extern uint8_t owi_IDs_pinMask[NUM_DEVICES]; /*Global variable to store the bus position corresponding*/

extern uint8_t BUSES[8];
//extern uint8_t BUSES_all[8];

//extern char PD;/*variable to check found devices*/
extern int8_t countDEV;/*number of devices (initialized to 0)*/
extern int8_t countDEVbus;/*number of devices on the current bus (initialized to 0)*/

extern uint8_t debug;
extern uint32_t debugMask;

enum debugLevels
{
   noDebug = 0,
   verboseDebug,
   eventDebug,
   eventDebugVerbose,
   periodicDebug,
   levelsDebug_MAXIMUM_INDEX
};

enum debugSystems
{
      debugMain,
      debugUART,
      debugCAN,
      debugTIMER0,
      debugTIMER1,
      debugTIMER0A,
      debugGETVOLTAGE,
      debugRELAY,
      debugCommandKey,
      debugOWI,
      debugOWITemperatures,
      debugDecrypt,
      debugDEBUG,
      debugOWIADC,
      debugOWIDualSwitches,
      debugOWISingelSwitches,
      debugSHOW,
      debugOWIApiSettings,
      debugSystems_MAXIMUM_INDEX
};

extern uint16_t owiBusMask;
extern uint16_t adcBusMask;

#endif

