#! Generated by VisualDCT v2.6.1280
#! DBDSTART
#! DBDEND



record(ao, "c_led$(port)") {
  field(DESC, "control pin output")
  field(DTYP, "stream")
  field(OUT, "@hadcon_RGWR.proto write($(register)) hadcon2")
}

#! Further lines contain data used by VisualDCT
#! View(2000,2115,1.0)
#! Record("c_led$(port)",2500,2361,0,1,"c_led$(port)")
