**Module: ACU System**

**Number:**

**Date: 17 August 2017**

**Tested by:**

**Destination:**

|  |  |
| --- | --- |
| General |  |
| Visual check of BKP cable connections |  |
| USI |  |
| USI 3 to 6 module connection check |  |
| USI 3 to 6 tripline/interlock check |  |
| SCU |  |
| Read at least one FSP content via SCU (\*) |  |
| DCCT |  |
| Check if the DCCT front LEDs are on connecting before the head to X1 |  |
| Power on the PC and check if a positive and negative current is displayed (\*\*) |  |

(\*) Don’t forget to unplug the USB cable used to connect PCA otherwise the SCU has not access to FSPs.

(\*\*) In order to display a current value as actual value, the MFU has to be configured properly.