# table of hadcon boards, detector and their position

|	hadcon     	|	detector |	position	|	devices                  | tasks  	
|	etrax239 	|	RPC		 |	sector I	|	1-wire: adc, temperature | Low voltage and Temperature	|
|	etrax203 	|	RPC		 |	sector II	|	1-wire: adc, temperature | Low voltage and Temperature	|
|	etrax210 	|	RPC		 |	sector III	|	1-wire: adc, temperature | Low voltage and Temperature	|
|	etrax232 	|	RPC		 |	sector IV	|	1-wire: adc, temperature | Low voltage and Temperature	|
|	etrax234 	|	RPC		 |	sector V	|	1-wire: adc, temperature | Low voltage and Temperature	|
|	etrax207 	|	RPC		 |	sector VI	|	1-wire: adc, temperature | Low voltage and Temperature	|
|   etrax231    |   MDC      |   hades		|	1-wire temperature       | Temperature					|
|   etrax237    |   MDC      |   hades		|	atmel adc                | relative Pressure			|
|   etrax201    |   MDC      |   hades		|	atmel adc and output     | pressure controlled relay	|
|   etrax236    |   ---      |   EE/KS	    |	---                      | development board        	|
|   etrax238    |   ---      |   EE/KS	    |	---                      | development board        	|
|   etrax247    |   ---      |   EE/KS	    |	---                      | development board        	|
|   etrax204    |   MDC      | L.F./sector Y|	CANbus                   | Wiener/HV Crate Control    	|
|   etrax243    |   MDC      | L.F./sector Y|	CANbus                   | Wiener/HV Crate Control    	|
|   etrax2xx    |   MDC      | L.F./sector Y|	CANbus                   | Wiener/HV Crate Control    	|
|   etrax2xx    |   MDC      | L.F./sector Y|	CANbus                   | Wiener/HV Crate Control    	|
|   etrax2xx    |   MDC      | L.F./sector Y|	CANbus                   | Wiener/HV Crate Control    	|
|   etrax2xx    |   MDC      | L.F./sector Y|	CANbus                   | Wiener/HV Crate Control    	|

