
Set fuses!

# olimex
avarice  -c 0,1,0,4 --jtag /dev/ttyUSB0 -B 1000000 -W ff19e0 
avarice  -c 0,1,0,8 --jtag /dev/ttyUSB0 -B 1000000 -W ff19e0 
# --> "make set_fuses" integrates this into Makefile

#mkII
avarice -2 -c 0,1,0,4 --jtag usb -B 1000000 -W ff19e0

